Mercury System

PB110

[IMAGE]

Relay Board - Product Datasheet

|  |  |
| --- | --- |
| Author | Francesco Ficili |
| Date | 03/03/2018 |
| Status | Draft |

|  |  |  |  |
| --- | --- | --- | --- |
| Revision History | | | |
| Version | Date | Author | Changes |
| 1.0 | 03/03/2018 | Francesco Ficili | Initial Release. |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

**SUMMARY**

[1. Introduction 4](#_Toc510204595)

[2. Block Diagram 6](#_Toc510204596)

[3. Hardware 8](#_Toc510204597)

[4. Pinouts 9](#_Toc510204598)

[Mercury Connector 9](#_Toc510204599)

[Programmer Connector 10](#_Toc510204600)

[Relay Connectors 10](#_Toc510204601)

[5. Command Set 12](#_Toc510204602)

[Specific Command Set 12](#_Toc510204603)

[Examples 12](#_Toc510204604)

[6. Technical Specifications 13](#_Toc510204605)

# Introduction

The Mercury System (MS in short) is a modular system for the development of connectivity and IoT applications. The system uses various type of electronic boards (logic unit, modems, slave board equipped with sensors and actuators, power boards...) and a complete SW framework to allow the realization of complex applications. Scalability, ease of use and modularity are key factors and are granted by the use of a heterogeneous set of components that allow to assemble the system like a construction made with LEGO© bricks.

The board set which composes the system is made up by the following “families”:

* **Base Board (BB):** It’s the “brain” of the system and contains the main logic unit as well as different communication buses and connector to interfaces the slaves. It also contains a simple power supply system and a recharge unit for a single LiPo cell (it can satisfy the power requirements of simpler systems). It can exist in different variants, depending on the employed microcontroller unit.
* **Modem Board (MB):** this one is the board that allow network connectivity. It can exist in different variant, depending on the network interface (GSM/GPRS, Wi-Fi, BT, Radio…). It’s interfaced to the Base Board with a dedicated serial line.
* **Power Board (PB):** it’s the board that allow to satisfy the particular power requirement of the system, when it’s necessary. They can be vary depending on the particular power requirement to satisfy (high power, solar harvesting, piezo harvesting, etc.).
* **Slave Board (SB):** these are the system’s peripherals, and they vary depending on the specific mounted sensor or actuator. Typical examples are SB with relay, temperature sensors, RGB LED controller, servo controller, accelerometer, etc. They communicate with the BB with I2C or UART and a dedicated command set.
* **Expansion Board (EB):** these are the board that allow planar connection of Mercury boards. There are variants which can contains Displays, battery socket, etc.
* **Brain-Less Board (BL):** these are the controller-less boards. They in general contain really simple sensor or actuators that don’t need the bus interface. There are meant as an alternative to slave boards for cost-sensitive applications.

Slave Boards and Modem Board are provided pre-programmed with a FW which implements a dedicated command set for a high-level management of the boards, while the Base Boards are provided with a SW framework which provides all the low-level services (operative system, device drivers, system services, etc.), leaving to the user only the development of application level logic. Moreover, the Base Board comes with an USB bootloader, so it can be programmed without the need of a flashing device.

Figure 1 shows a typical system connection:




Figure 1 - Typical System Connection

Examples of application fields of MS are:

* Home automation System,
* IoT applications,
* Connectivity Applications,
* Monitoring and control Systems,
* Remote Control,
* Industrial Process control,
* Robotics applications,
* Test benches,
* Etc…

# Block Diagram

The SB110 is a 2-channel Relay board, able to control load up to 1A per channel. Figure 2 shows the SB110 block diagram. The heart of the system is a PIC16F1825 8-bit RISC microcontroller, produced by Microchip Technology Inc.




Figure 2 - Block Diagram

The main characteristics of the employed MCU are resumed in Table 1:

Table 1 - MCU characteristics

|  |  |
| --- | --- |
| Parameter Name | Description |
| Program Memory Type | Flash |
| Program Memory (KB) | 14 |
| CPU Speed (MIPS) | 8 |
| RAM Bytes | 1,024 |
| Data EEPROM (bytes) | 256 |
| Digital Communication Peripherals | 1-UART, 1-A/E/USART, 1-SPI, 1-I2C1-MSSP(SPI/I2C) |
| Capture/Compare/PWM Peripherals | 2 CCP, 2 ECCP |
| Timers | 4 x 8-bit, 1 x 16-bit |
| ADC | 8 ch, 10-bit |
| Comparators | 2 |
| Temperature Range (C) | -40 to 125 |
| Operating Voltage Range (V) | 1.8 to 5.5 |
| Pin Count | 14 |
| XLP | Yes |
| Cap Touch Channels | 12 |

The SB110 is connected to the BB by means of I2C bus. The address of the board could be dynamically set by means of a 4 positions dip switch, allowing up to 15 address values (address 0x00 is reserved for I2C general call broadcast addressing scheme).

Table 2 resumes the SB110 board main characteristics:

Table 2 – Board Characteristics

|  |  |  |
| --- | --- | --- |
| Parameter | Description | Notes |
| Board Type | Slave Board (SB) |  |
| Supported Bus | I2C |  |
| Addressing | Dip Switch 4 |  |
| Peripheral Description | 2 Relay Channels | Sanyou SYS-S-105L |

# Hardware

This section goes deeper in the HW details of SB110. Figure 3 depicts the most important components of the board:




Figure 3 - Hardware Highlight

Table 3 provides a description of board’s main components:

Table 3 –Hardware characteristics

|  |  |
| --- | --- |
| Name | Description |
| User LED | Board User LED, by default it’s configured as heartbeat LED (periodic pulses). |
| Relays | The SB110 is equipped with two Sanyou miniature relays model SYS-S-105L. |
| Relay Outputs | Output Relays connectors. |
| Mercury Connector | Mercury connector used to interface the board with the others MS boards. |
| Address Dip Switch | Dip Switch to set the address of the board within the Mercury System. |
| MCU | PIC16F1825 main controller board. |
| Programmer Connector | PicKit 3 Microchip Programmer/debugger connector. It is directly connected to the MCU debug port, in order to allow advanced debugging and programming features, if needed. |

# Pinouts

This section highlights the pinouts of SB110 connectors.

## Mercury Connector

The Mercury Connector is the connector which interfaces the SB110 with the rest of Mercury System. The connector’s pinout is depicted in Figure 4 and Table 4 explains the meaning of each single pin (NC stands for “Not Connected”).

Table 4 - Mercury Connector Pinout

|  |  |  |
| --- | --- | --- |
| Pin Name | Pin Number | Description |
| VddBat | CN1 – 1  CN2 – 2 | This pin is connected to the main power source and is used as main source to drive relays coil. |
| VddMcu | CN1 – 2 | This pin is connected to MCU regulated positive voltage reference (3,3V). |
| GND | CN1 – 3  CN2 – 1 | This pin is connected to the board reference voltage. |
| SDA | CN2 – 7 | This pin is connected to I2C SDA line (Data Line). |
| SCL | CN2 – 8 | This pin is connected to I2C SCL line (Clock Line). |




Figure 4 - SB110 Mercury Connector Pinout

## Programmer Connector

The Programmer Connector is the connector which allows to re-program the SB110 using Microchip Technology ICSP (In-Circuit Serial Programming) interface. The connector’s pinout is depicted in Figure 5 and Table 5 explains the meaning of each single pin (NC stands for “Not Connected”).

Table 5 - Programmer Connector Pinout

|  |  |  |
| --- | --- | --- |
| Pin Name | Pin Number | Description |
| MCLR | CN3 – 1 | Microcontroller Master Clear (RESET) pin. |
| Vdd | CN3 – 2 | Positive power supply reference. |
| GND | CN3 – 3 | Negative power supply reference. |
| PGD | CN3 – 4 | Program Data pin. |
| PGC | CN3 – 5 | Program Clock pin. |




Figure 5 - SB110 Programmer Connector Pinout

## Relay Connectors

The Relay Connectors interface the SB110 onboard relays. The connector’s pinout is depicted in Figure 6 and Table 6 explains the meaning of each single pin.

Table 6 - Relay Connectors pinout

|  |  |  |
| --- | --- | --- |
| Pin Name | Pin Number | Description |
| NC | CN4,5 – 1 | Normally closed relay output. |
| C | CN4,5 – 2 | Common relay output. |
| NO | CN4,5 – 3 | Normally open relay output. |




Figure 6 - SB110 Relay Connectors pinout

# Command Set

## Specific Command Set

The SB110 board supports both the MS Generic Command Set (see document MS\_SlavesGenericCommandSet) and a set of specific commands (also called Specific Command Set).

Table 7 lists the SB110 Specific Command Set:

Table 7 - Command Set

|  |  |  |  |
| --- | --- | --- | --- |
| Code | Cmd Name | Parameters | Description |
| 0x50 | Set Relay Status | RelaySts (1 byte) | Set the status of relays. The relay status is mapped as bitfield in the RelaySts parameter (each bit represents a relay channel, only the first two bits are used.) |
| 0x51 | Impulse Relay1 Seconds | ImpulseLen (2 byte) | Generates an impulse of duration equal to ImpulseLen for relay 1 (ImpulseLen parameter is in seconds). |
| 0x52 | Impulse Relay2 Seconds | ImpulseLen (2 byte) | Generates an impulse of duration equal to ImpulseLen for relay 2 (ImpulseLen parameter is in seconds). |
| 0x53 | Impulse Both Relays Seconds | ImpulseLen (2 byte) | Generates an impulse of duration equal to ImpulseLen for both relays (ImpulseLen parameter is in seconds). |
| 0x60 | Request Relays Status | None | Request the relays current status. This command prepares one byte which represents the status of relays as bitfield in the response buffer, an I2C read request must be issued to read the prepared value. |

## Examples

Some examples of Specific Command Set usage are listed below:

1. Set of Relay1 output On and Relay2 output Off: **[0x50] [0x01]**
2. Set of Relay1 output Off and Relay2 output On: **[0x50] [0x02]**
3. Set of Both Relays Outputs On: **[0x50] [0x03]**
4. Generate 10s impulse on Relay1 channel: **[0x51] [0x0A]**
5. Generate 5s impulse on Relay2 channel: **[0x52] [0x05]**
6. Request Relays status: **[0x60] + Read Operation on I2C bus**

# Technical Specifications

Table 8 resumes the board technical specifications:

Table 8 - Board Technical Specifications

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Parameter | Max | Typ | Min | Unit | Notes |
| Supply Voltage | 3.6 | 3.3 | 2.0 | V |  |
| Current Cons. (Normal) |  | 10 |  | uA |  |
| Current Cons. (Peak) |  | 1 |  | mA |  |
| Current Cons. (Low Power) |  | 100 |  | nA |  |
| Startup Time |  | 100 |  | mS |  |
| Output Ch. Max Current | 1 |  |  | A | Each channel. |